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  SCHEDA TECNICA ELETTROVALVOLA 18025 3/4”
	DESCRIZIONE

	Elettrovalvola 2/2 vie Normalmente Chiusa (NC)



	CARATTERISTICHE MECCANICHE



	MATERIALE CORPO
	Stampato ottone                                     ST-UNI EN12165-CW617N (OT58)

	INGRESSO
	Filetto femmina G3/4”

	USCITA
	Filetto femmina G3/4”

	NUCLEI
	Acciaio inossidabile ferromagnetico

	GUARNIZIONI
	NBR / EPDM / Viton

	ORIFIZIO INGRESSO (DN)
	(18.0 mm

	TAMBIENTE  MASSIMA (certificazione VDE)
	
	80 °C

	TFLUIDO  MASSIMA (compatibile con NBR)
	
	120 °C

	PESERCIZIO MASSIMA con ARIA

(bobina a temperatura ambiente)
	
	15 bar

	PESERCIZIO MASSIMA con ACQUA

(bobina a temperatura ambiente)
	
	15 bar

	PINVERSA   MASSIMA (sull’uscita)
	
	0,1 bar

	Portata d'acoua a TAMBIENTE  ((P=1 bar):
	
	5,0 m³/h

	CARATTERISTICHE ELETTRICHE


	CLASSE DI ISOLAMENTO ELETTRICO
	I

	CLASSE DI TEMPERATURA
	H

	CLASSE DI PROTEZIONE (senza connettore DIN43650-B)
	IP00

	CLASSE DI PROTEZIONE (con connettore DIN43650-B)
	IP65

	TENSIONE ALIMENTAZIONE
	230 Vac 50 Hz ((10%)

	POTENZA (a freddo)
	12.3 VA

	POTENZA (a caldo)
	9 VA

	TIPO DI SERVIZIO
	Continuo (ED100%)


	Data:
	22-01-2007

	Rev.
	07/1

	Compilato da:
	G. BUCCIO


DATA SHEET FOR SOLENOID VALVE 18025 3/4”
	DESCRIPTION

	Solenoid valve 2/2 ways slow closing servo-controlled ( NC )


	MECHANICAL CHARACTERISTICS


	BODY MATERIAL
	Forged brass                                          ST-UNI EN12165-CW617N (OT58)

	INLET
	Female thread G3/4”

	OUTLET
	Female thread G3/4”

	PLUNGERS
	Magnetic stainless steel

	GASKETS
	NBR / EPDM / Viton

	INPUT ORIFICE (DN)
	(18.0 mm

	TROOM  MAXIMUM (VDE certification)
	
	80 °C

	TFLUID  MAXIMUM (according with NBR)
	
	120 °C

	PWORKING  MAXIMUM with AIR
(coil at room temperature)
	
	15 bar

	PWORKING  MAXIMUM with WATER
(coil at room temperature)
	
	15 bar

	PREVERSE   MAXIMUM (at the output)
	
	0,1 bar

	Flow rate with water at TROOM  ((P=1 bar):
	
	5,0 m³/h

	ELECTRICAL CHARACTERISTICS



	ELECTRICAL INSULATION CLASS
	I

	TEMPERATURE CLASS
	H

	PROTECTION CLASS (without connector DIN43650-B)
	IP00

	PROTECTION CLASS (with connector DIN43650-B)
	IP65

	POWER SUPPLY
	230 Vac 50 Hz ((10%)

	POWER (at room temperature)
	12.3 VA

	POWER (at hot temperature)
	9 VA

	TYPE OF SERVICE
	Continuos (ED100%)


	Date:
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	Rev.
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	Filled out by:
	G. BUCCIO
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