Datasheet Rope pull switch 
	Description:
	SZS SU1
	Article number:
	8038 0010
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Wiring diagram:

	Design
	Rope pull switch, with signal tower and connector

	
	

	Microswitch
	

	Voltage

	24 V DC

	Current capacity

	max. 100mA

	Mechanical life
	min.10 Mio.

	Switch function
	Momentary switch 

	Contact material
	Gold alloy

	Switch type
	1 NO contact

	Switching system
	Snap action

	
	

	LED Unit
	

	Rated voltage
	24V DC ±10% (21,6 - 26,4V DC)

	Current / Power
	52mA / 1,25W

	LED Unit color
	Amber

	
	

	Traction force
	in axial direction ca. 80-130 N

	Forerun
	ca. 2mm

	Switching distance
	ca. 10mm

	
	

	Housing
	Mold casting, powder-coated RAL 7035 (light grey)

	Cover
	Mold casting, powder-coated RAL 7035 (light grey)

	Spring bush
	Mold casting, powder-coated RAL 7035 (light grey)

	Actuator
	Ring eyelet (steel, zinc-plated) not rotatable, inside ø 20mm, outside ø 36mm

	Assembly
	4x M6 (see Drawing)

	Connection
	5 pin-connector M12

	
	

	Cable entry
	2x M20x1,5 outlets lateral

	
	

	Protection type
	IP54 acc. to IEC/EN 60529

(If cover is closed and use an equivalent cable gland with adequate cable)

	Ambient air temperature
	-20°C to +80°C

	
	

	Regulations
	IEC/EN 60204

IEC/EN 60947-5-1
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