Description: MOTOX bevel gear
Type: K108-A160X
MLFB: ST31506-1JA00-0AJ1-Z
Short details: K01+D08+L03+L50+K06+K19+A00+A15
Customs tariff number: 84834023

Engine options
Electrical design: CE
Motor rotation direction: right

Clutch options
AV unit: A160X
AV: Sealing: Normal
Drive shaft: V42 x 110

Gearbox options
Gearbox: K108
Output rotation direction: left
Bearing: assigned bearing
Ratio: 23.08
Gearbox housing material: GG
Gearbox output torque: 2262
Output seal: Normal
Output shaft: V60 x 120
Shaft material: 42CRMO4
Shaft cover: Cover cap
Number of sealing rings: 1
Relubrication unit: without
Oil type 1: CLP VG220
Oil quantity 1: 6.20
Ventilation: Vent filter
Oil drain: Oil drain screw
Oil level control: Oil level screw
Drywell version: without
Bevel gear position: N388.05

General options
Design: B3-00-B
Backstop: YES
Backstop rotation direction: right
Protection class: IP55
Rating plate: Steinlen
Color: 5015
Paint code: C2
Weight: 166.00
Ambient temp.: -20 ... +40 °C

Factory standards
Factory standards 1: N738.05

Operating instructions
Adapter operating instructions: BA2019
[bookmark: _GoBack]Gearbox operating instructions: BA2010
