Product information
Fieldpiece offers state-of-the-art Digital Manifolds.

- Supports A1, A2L and A3 refrigerants;

- Can be integrated with Job Link® tools;

- Temperature compensated system tightness test;

- Heavy-duty weatherproof design.

Our Digital Manifold can work with complex HVACR systems and integrate with Job Link® tools, so you have all the information you need in the palm of your hand.

Four reasons why you need the SM480VINT

1. Integrate with Job Link® tools
The wireless SM480VINT is the heart of every job as the Digital Manifold. All Job Link® tools can be connected to the SM480VINT and with a wireless range of 300 m you will find real-time, accurate measurements from all Job Link® tools directly on your Digital Manifold. The on-board data recording function (up to 7 days) streamlines your work and ensures you can give customers all the answers they need.

2. Support for A1, A2L and A3 refrigerants
The SM480VINT is designed to work with A1, A2L and A3 refrigerants and blends to comply with F-gas regulations. This high-tech Digital Manifold not only helps you do your work easier, faster and better, but also supports the environment.

3. Reliable and accurate
Thanks to the temperature-compensated system tightness test, you never have to worry about inaccurate measurements. Plus, the built-in vacuum gauge provides you with all the vacuum-related information you need.

4. Robust design
Robust and reliable. The heavy housing, reinforced hook, IP54 waterproofing and shock-resistant illuminated screen ensure that the SMAN® can withstand all conditions, so that you can continue to do your work easier, faster and better.

To connect the SR47INT or SR47EC to your SMAN® Digital Manifold, make sure you are using the latest software.

Specifications

Display: LCD (12.7cm diagonal)
Backlight: Blue (adjustable duration)
Low Battery Indication: Displayed when the battery voltage drops below operating level.
Auto shut-off: 30 minutes of inactivity (adjustable)
Maximum inlet pressure: 800 Psig (5500 kPa)
Battery type: 6 x AA alkaline
Battery life: average 350 hours (without vacuum, backlight and wireless)
Radio frequency: 2.4 GHz
Wireless range: 300 meters line of sight
Distance decreases due to obstructions
Data Port: Micro USB (for retrieving data logs or updating firmware)
Operating environment: 0°C to 50°C at <75% RH
Storage environment: -20°C to 60°C at <80% RH (with battery removed)
Temperature coefficient: 0.1 x (specified accuracy) per °C (0°C to 18°C, 28°C to 50°C)
Weight: 1.83kg
Water resistant: Designed to IP54

Included in packaging

SM480VINT
(2) TC24 wired type K pipe clamp thermocouple
(1) ATA1 Type-K type bead thermocouple with clip
(1) ANC11 Padded storage bag