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�
�
Motor�
�
�
�
Frequency�
Hz�
50�
�
Shaft speed�
min-1�
1500�
�
Voltage�
V�
3~400�
�
Input power�
VA�
33,9�
�
Output power�
W�
15,4�
�
Total resistance�
Ω�
4155�
�
Starting voltage�
V�
260�
�
No-load current�
mA�
50�
�
Current input�
mA�
65�
�
Torque at the motor shaft�
cN·m�
9,8�
�
Operation mode�
S1�
100%�
�
Protection class�
IP�
40�
�
Temperature class�
�
B�
�
Connection type�
�
leads�
�
Gear�
�
�
�
Transmission�
i�
1000:1�
�
Housing�
�
zinc�
�
Rated torque�
cN·m�
5000�
�
Permissible output torque max.�
cN·m�
1000�
�
Shaft speed�
rpm�
1�
�
Shaft diameter�
mm�
8�
�
Shaft length from flange�
mm�
25�
�
Shaft execution�
�
With flat 7x21 mm�
�
Dimensions�
�
�
�
Motor diameter�
mm�
65�
�
Gear diameter�
mm�
65�
�
Length motor - gear�
mm�
109±1�
�
Weight motor – gear �
gr�
approx. 1100�
�










































Synchronous geared motor
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