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MOTOR PART NR
	
OH090S4
	
CUSTOMER PART NR
	


	DRAWING NR
	OH090S4
	MOTOR TYPE
	OH090S A4

	Type of winding
	3 PHASE 1 SPEED 6 LEADS
	EFFICIENCY IE
	IE3
	4/4
	3/4
	1/2

	
	
	
	
	84,1
	84,1
	81,6

	PROTECTION 
	II 2G Ex db IIC T4 Gb 
	CERTIFICATE
	EPT 17 ATEX 2588X

	IP PROTECTION
	IP66
	ENVIRONMENT CONDITIONS
	-20 /+50°C Max Altitude: 1000m

	POLES
	4
	NOMINAL POWER kW
	1,10


	Nom. Speed rpm
	1440
1735
	Voltage-Frequency
	230/400V 50Hz
265/460V 60Hz
	Tolerance:  Voltage  ±5%

	Nom. Current  A
	4,52/2,61
4,52/2,61
	COS 
	0,724
0,724

	Starting current / Rated current 

	6,6
	Starting torque /
Rated torque 
	2,8

	Breakdown torque/ Rated torque 

	2,8
	Weight 

	16

	Duty
	S1 Continuous Duty
	Direction of Rotation
	BIDIRECTIONAL

	Insulation Class
	F 
	Mounting IM
	B3

	IEC Frame Size
	90
	Material end Shield/Flange
	Aluminium

	Material Terminal Box
	Aluminium
	Material Fan
	Plastic

	Material Cover Fan
	Zinc plated steel
	Material shaft
	Steel C43 

	DE Bearing Type
	6205-ZZ  
	NDE Bearing Type
	6205-ZZ

	Position of terminal box
	TOP
	Cable gland Type
	M20x1,5

	Cable gland position (view from DE)
	Right
	Thermal protection
	

	Painting 
	
	Motor Colour
	


       
	In compliance with the EC Directives
	and comply with the following Standards

	2014/34/UE 	(ATEX)
2014/30/UE 	(EMC)
2006/42/EC	(Machinery)
2011/65/CE	(RoHS II)

	EN 60079-0, 
EN 60079-1, 31
EN 60034-1,2,5,6,7,9,12,14, 
IEC60072-1, 
 EN 60259


Overall dimensions (mm)
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	B 
	A 
	HA 
	BB 
	AB 
	AC 
	AD 
	AP
	AF 
	C 
	H 
	HD 
	LB 
	LR 
	L 
	K1 
	K2
	MC
	D 
	E 
	GA 
	F 
	DB 

	100
	140
	14,5
	130
	170
	176
	174
	119
	119 
	57
	90
	264
	270
	283
	320
	10
	17,5
	M20 
	24
	50
	27
	8
	M8X19



	La O1EM S.p.A. si riserva a termini di legge la proprietà del documento con divieto di riprodurlo o di renderlo comunque noto a terzi o a ditte concorrenti, senza la sua autorizzazione.
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