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D27300 
MACHINERY PLANER THICKNESSER 2800W

OVERVIEW
· High quality, robust design
· No-volt release switch, motor overload protection and cutter block guard for safe working
· Large, extruded aluminium top planing table for high accuracy and ease of use
· Integrated motor design to save space and improve transportation
· New control design to improve ease of use and accuracy of adjustment
· Large aluminium fence for accurate bevel angles in the surface planing mode
· 100 mm dust extraction port for a clean, safe working environment
· Micro switch attached on the gaurd to prevent accidental operation when the gaurd is not in place
 (
S
tandard
HSS knives
Adjustable fence
Allen keys
Spanner
Blade setting gauge
Dust extraction mouthpiece
Push stick
Legset
)Specificatii
	Power Input
	2100 Watts

	Power Output
	1600 Watt

	No Load Speed
	6200 rpm

	Max. Capacity
	260 mm

	Max. Depth of Cut
	4 mm

	Max. Planing Depth
	3 mm

	Planer Table Size
	1000 × 260 mm

	Thicknesser Table Size
	500 × 250 mm

	Max. Thicknesser Capacity
	160 mm

	Feed Rate
	5 m/min

	Weight
	53 kg

	Depth
	700 mm

	Length
	1050 mm
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