PROGRESSIVE CAVITY PUMP

Type: MDC 025 -6L /J0-A7-A7-R0-G60-X

Kind of Installation;   Horizontal

Commision No. :   251798

Manufacturer:       seepex GmbH
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Drive

Type               geared motor
Make             Getriebebau Nord ratio i= 5,530
Model            SK0XF-71L/4
Mounting position        IMB3/B5 nom./ min- max
Flange dia           120 mm                                                    Output speed      250/ 62- 271 rpm
output shaft          716/M120-001B4                 Motor speed 1380/ - rpm
Frequency            50/ 12- 54 Hz
Type of adjustment           frequency control
Electric Motor            0.37kw
